






ORDER

№ A 267

Sofia, 04.07.2023


KVL-KNYAZHEVO-KOPITOTO EOOD, SOFIA

INSPECTION BODY OF TYPE С „CC-BRC"


Management and office address: 1415 Sofia, Dragalevtsi r. q., 51 Krushova Gradina str.



To perform inspection of:

	Type of scope: flexible*

	
№

	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1.
	Ropes for: ropeways, ski lifts, lifting equipment, elevators, shafts and similar equipment 
	New facilities and/or units in use/operation (equipment) 
	Broken and loose wires, wear and corrosion
	Magnetic (magneto-inductive) control method Methodology № KK- БРК-10
БДС EN 12927



	Ordinance on the safe operation and technical supervision of ropeways, SG (State Gazette, Bulgaria) issue 58/2014
БДС EN 12927
TC

	
	
	
	
	Visual control method
Methodology № KK-БРК-6
БДС EN 13018
	Ordinance on the safe operation and technical supervision of ropeways, SG. issue 58/2014
БДС EN 12927
ТС

	2.
	Cable lines, ski tows, details and assemblies
	New sites/facilities and/or ones in use/operation
	Type, size and location of problems (imperfections)
	Ultrasonic control method - Methodology № KK-БРК 1
БДС EN ISO 16810 
БДС EN 10228-3
	Ordinance on the safe operation and technical supervision of ropeways, SG issue 58/2014
ТС

	
	
	
	Type, size and location of problems (imperfections)
	Magnetic (powder) method for control Methodology № KK-БРК 3
БДС 7156
БДС EN 10228-1
БДС EN ISO 9934-1 БДС EN ISO 3059
	Ordinance on the safe operation and technical supervision of ropeways, SG  issue 58/2014
БДС EN 10228-1 ТС

	
	
	
	Type, size and location of problems (imperfections)
	Control method using penetrating liquids 
Methodology № KK-БРК 5
БДС EN 10228-2
БДС EN ISO 3452-1 БДС EN ISO 3059
	Ordinance on the safe operation and technical supervision of ropeways, SG  issue 58/2014
БДС EN 10228-2 ТС

	
	
	
	Type, size and location of problems (imperfections)
	Visual control method 
Methodology № KK-БРК 6 
БДС EN 13018
	Ordinance on the safe operation and technical supervision of ropeways, SG issue 58/2014
ТС

	3.
	Facilities, constructions and elements – basic metal and welded joints 
	New facilities and/or units in use/operation (equipment)
	Type, size and location of problems (imperfections)
	Magnetic (powder) control method  Methodology № KK-БРК 4 
БДС 15575
БДС EN ISO 17638
	БДС EN ISO 23278
БДС EN ISO 5817
ТС

	
	
	
	Type, size and location of problems (imperfections)
	Control method using penetrating liquids 
Methodology
№ KK-БРК 5
БДС EN ISO 3452-1
	БДС EN ISO 23277
БДС EN 10228-2 БДС EN ISO 5817
ТС

	
	
	
	Type, size and location of problems (imperfections)
	Visual control method 
Methodology № KK-БРК 7 
БДС EN ISO 17637
	БДС EN ISO 5817 ТС

	
	
	
	Type, size and location of problems (imperfections)
	Ultrasound control method Methodology № KK-БРК 1
БДС EN ISO 16810
БДС EN ISO 17640
	БДС EN 10228-3
БДС EN ISO 11666
БДС EN ISO 23279
БДС EN ISO 5817
ТС

	4.
	Metal facilities 
	New facilities and/or units in use/operation (equipment)
	Thickness of walls – one-sided access 
	Ultrasound control method Methodology № KK БРК 2
БДС EN ISO 16810
БДС EN ISO 16809
	Technical specifications  

	5.
	Electrical units and facilities (up to 1000 V)
	New facilities and/or units in use/operation (equipment)
	Resistance of protection/ grounding units 
	Control procedure № KK-БРК 8 А
	Ordinance № 3, SG issue  90-91/2004 Ordinance № 16-116 (SG issue 26/2008)

	
	
	
	Impulse resistance of lightning protection grounding systems
	Control procedure № KK-БРК 8
	Ordinance № 4, SG issue  6/2011
 

	
	
	Impedance Zs for phase contour – safety contour 
	Control procedure № KK-БРК 9
	Ordinance № 3/ 2004, SG issue  90- 91/2004
Ordinance № 16-116, SG issue 26/2008



* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the CAB.

Ordinance on the safe operation and technical supervision of ropeways. SG issue 58/2014; 
Ordinance № 16-116 on the technical operation regarding power equipment (prom. in SG, issue 26/2008);
Ordinance № 3 on the arrangement of electrical equipment and power lines (prom. in SG, issue 90/2004, issue 91/2004, amended in SG issue 108/2007); 
Ordinance № 4/2010 on the lightning protection of buildings, outdoor facilities and open spaces (SG issue 6/18.01.2011);
TC – Technical specification.
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