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№ A 496

Sofia, 01.12.2023

“DIA KONSULT 8” LTD
INSPECTION BODY OF TYPE С
 

Registered office: 6343, Mineralni Bani village, Haskovo region, 16 Hristo Botev Blvd.
Office address: 6300, Haskovo, 17 Klokotnitsa St.


To perform inspection according to the following scope:

	Scope type: flexible*

	№
	Field of inspection
	Type of inspection
	Parameter of Inspection/ Characteristic
	Test and Measurement Methods Used During Inspection, Inspection Procedure
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	
1
	Electrical systems and equipment of up to 1000V and above
	Initial /periodic of new and/or in operation sites/ equipment
	Resistance of protective earthing systems
	RP7.1.1.1; Ordinance №RD-02-20-1, SG № 53/2018
	Ordinance № 3,SG № 90 and 91/2004; Ordinance № 16-116, SG № 26/2008; 
БДС 3820; TS

	
2
	Electrical systems and equipment of up to 1000V and above

	Initial /periodic of new and/or in operation sites/ equipment
	Resistance of lightning protection earthing systems
	RP7.1.1.2; Ordinance №RD-02-20-1, SG № 53/2018
	Ordinance № 3, SG № 90 and 91/2004; Ordinance № 4, SG № 6/2011;
Ordinance № 16-116, SG № 26/2008; TS

	
3
	Electrical systems and equipment of up to 1000V

	Initial /periodic of new and/or in operation sites/ equipment
	Insulation resistance
	RP7.1.1.3; Ordinance №RD-02-20-1, SG № 53/2018; 
БДС 1986 p. 3.3. a,b,c,d
	Ordinance № 3, 
SG № 90 and 91/2004;
Ordinance № 16-116, SG № 26/2008; Ordinance № RD-02-20-1, SG № 53/2018; TS

	4
	Electrical systems and equipment of up to 1000V

	Initial /periodic of new and/or in operation sites/ equipment
	Loop impedance "Phase-" protective conductor
	RP7.1.1.4; Ordinance №RD-02-20-1, SG № 53/2018; 
	Ordinance № 3, 
SG № 90 and 91/2004; 
Ordinance № 16-116, SG № 26/2008; TS

	
5
	Electrical systems and equipment of up to 1000V - Safety switches

	Initial /periodic of new and/or in operation sites/ equipment
	Shutdown time; Trigger current; Touch voltage; Resistance of protective earth
	RP7.1.1.5; Ordinance №RD-02-20-1, SG № 53/2018; 
	Ordinance № 3, 
SG № 90 and 91/2004; 
Ordinance № 16-116, SG № 26/2008; Ordinance № RD-02-20-1, SG № 53/2018; TS

	
6
	Physical factors - Noise in the working environment

	Initial /periodic of new and/or in operation sites
	Daily noise exposure level; Peak sound pressure level; Average weekly noise exposure level; Noise level; Equivalent noise level
	RP7.1.1.6; 
БДС EN ISO 9612;
(БДС ISO 1999); 
БДС 15471 
	Ordinance № 6, 
SG № 70/2005; 
Ordinance № 7, 
SG № 88/1999; 
Ordinance № 9, 
SG № 46/1994; 
TS

	
7
	Physical factors - Noise in the premises of residential and public buildings


	Initial /periodic of new and/or in operation sites
	Noise level; Equivalent noise level
	RP7.1.1.7; 
БДС 15471 
	Ordinance № 6 (Appendix № 2, Table 1), SG № 58/2006; Ordinance № 2, 
SG № 15/2007; 
Ordinance № 9, 
SG № 46/1994; 
Ordinance № 24, 
SG № 95/2003; 
Ordinance № 26, 
SG № 103/2008; Ordinance № RD-02-20-3, SG № 5/2016; TS

	
8
	Physical factors - 
Artificial lighting in working environments, premises of residential and public buildings 


	Initial /periodic of new and/or in operation sites
	Illumination/ Lighting
	RP 7.-1.1.8; 
MGMEAL 40-85, ed."Standardization", 1985

	Ordinance № 49, 
SG № 7/1976; Ordinance № 2, SG № 15/2007;
Ordinance № 3, 
SG № 15/2007;
Ordinance № 9, 
SG № 46/1994;
Ordinance № 24, 
SG № 95/2003;
Ordinance № 26, 
SG № 103/2008;
Ordinance № RD-02-20-3, SG № 5/2016; БДС EN 12464-1; 
БДС EN 12464-2; 
TS

	
9
	Physical factors - Microclimate in the working environment, premises of residential and public buildings


	Initial /periodic of new and/or in operation sites/ equipment
	Air temperature; Relative air humidity; 
Air movement speed
	RP 7.-1.1.9; 
БДС 16686; Ordinance №RD-07-3, 
SG № 63/2014
	Ordinance № RD-07-3, SG № 63/2014; Ordinance №RD-02-20-3, SG № 5/2016; Ordinance № 2, 
SG № 15/2007;
Ordinance № 3,
SG № 15/2007;
Ordinance № 7, 
SG № 88/1999; 
Ordinance № 9, 
SG № 46/1994; 
Ordinance № 24,
SG № 95/2003; Ordinance № 26, 
SG № 103/2008;
БДС 14776;
TS

	
10
	Physical factors –
Air conditioning installations

	Initial /periodic of new and/or in operation sites/ equipment
	Air temperature; Relative air humidity
	RP 7.1.1.10; 
БДС 16686; Ordinance №RD-07-3, 
SG № 63/2014
	Ordinance № 15, 
SG № 68/2005; Ordinance № RD-07-3, SG № 63/2014; Ordinance № RD-02-20-3, SG № 5/2016;
БДС 14776;
TS

	
11
	Physical factors –
Ventilation installations
	Initial /periodic of new and/or in operation sites/ equipment
	Air flow velocity; 
Air flow rate
	RP 7.1.1.11; 
БДС 12.3.018
	Ordinance № 15, 
SG № 68/2005; Ordinance № 24, 
SG № 95/2003; Ordinance №
RD-02-20-3, 
SG № 5/2016; 
TS

	
12
	Chemical factors - Chemical agents in the workplace 

	Initial and/or periodic on new and/or in use/operation sites
	Concentration of chemical agents in the air by linear colorimetric method
	RP 7.1.1.12; 
БДС EN 482; 
БДС EN 689 +AC
	Ordinance № 13, 
SG № 8/2004; 
Ordinance № 10, 
SG № 94/2003; 
TS

	
13
	Chemical factors - Dust in the workplace

	Initial and/or periodic on new and/or in use/operation sites
	Concentration of dust in air: Inhalable fraction; Respirable fraction
	RP 7.1.1.13; 
БДС EN 482; 
БДС EN 689 +AC
БДС 2200
	Ordinance № 13, 
SG № 8/2004;
Ordinance № 10, 
SG № 94/2003;
TS



* The introduction of a new version of standards/documents or standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the Conformity assessment bodies.

Ordinance № 3 on the design of electrical systems and power lines (SG № 90 and 91/2004); 
Ordinance № 16-116 on the technical operation of electrical equipment (SG № 26/2008); 
Ordinance № 4 on the lightning protection of buildings, outdoor facilities and open spaces (SG № 6/2011); 
Ordinance № RD-02-20-1 of 2018 on technical rules and regulations for control and acceptance of electrical installation works (SG № 53/2018);
Ordinance № 6 on the minimum requirements for provision of health and safety of workers against risks involving noise exposure (SG № 70/2005); 
Ordinance № 7 of 1999 on the minimum requirements for health and safety at Work and upon use of working equipment (SG № 88/1999); 
Ordinance № 9 on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students (SG № 46/1994);
Ordinance № 6 of 2006 on the environmental noise indicators, taking into account the degree of discomfort during the different parts of the day, the limit values of the environmental noise indicators, in the premises of residential and public buildings, in zones and territories intended for residential construction, recreational areas and territories and mixed-use areas, the assessment methods of the noise indicator`s values and the harmful effects of noise on public health (amend. title – SG № 100 of 2021) (SG № 58/2006);
Ordinance № 2 of 2007 on the health requirements for computer and Internet rooms for public use (SG № 15/2007); 
Ordinance № 24 - on sanitary and hygienic requirements for discotheques (SG № 95/2003); 
Ordinance № 26 of 2008 on the structure and activity of nurseries and children’s kitchens and the health requirements towards them (SG № 103 / 2008);
Ordinance № RD-02-20-3 of 2015 on the design, implementation and maintenance of public service buildings in the field of education and science, health care, culture and the arts (SG № 5 / 2016); 
Ordinance № 49 - on the artificial lighting of buildings (SG № 7/1976);
Ordinance № 3 of 2007 on health requirements for kindergartens (SG № 15/2007); 
Ordinance № RD-07-3 - on the minimum requirements regarding the microclimate of workplaces (SG № 63/2014);
Ordinance № 15 - on the technical rules and standard specifications for design, construction and operation of the facilities and installations for the production, transmission and distribution of thermal energy (SG № 68/2005);
Ordinance № 13 of 2003 on the protection of workers from risks related to exposure to chemical agents at work (SG № 8 / 2004); 
Ordinance № 10 of 2003 on the protection of workers from risks involving exposure to carcinogens and mutagens at work (SG № 94 / 2003); 
MGMEAL 40-85. Methodological guidelines for measuring and evaluating artificial lighting in buildings 40-85, ed. Standardization, 85;
TS - Technical specification of the client.

Page 4 of 4


