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ORDER 
No. A 185
Sofia, 28.04.2023

INSPECTION BODY OF TYPE C

at “CTM 2002”Ltd., KUSTENDIL

Management address: 2500, The city of  Kustendil, 22 Rakovska street, Block 4, Apartment 67
Office address: 2500, The city of Kustendil, 2 Macedonia Square /NTS/, Floor 2, Room 2
To perform inspection of:
	Scope type: Flexible

	№

	Field of Inspection
	Type of Inspection
	Parameter of Inspection / Characteristic
	Test and Measurement Methods Used During Inspection
	Regulations, Standards, Specifications, Schemes

	1
	2
	3
	4
	5
	6

	1
	Microclimate in working and household environment
	New and/or operational sites/facilities
	Air temperature; Relative humidity; Air velocity and movement
	БДС 16686-87
Ordinance No. РД-07-3, State Gazette (SG), issue 63/2014
01-M Procedure on microclimate control

	Ordinance No 2, SG, issue 15/2007;
Ordinance No 9, SG, issue 46/1994;
Ordinance No 24, SG, issue 95/2003;
Ordinance No 3, SG issue 15/2007;
Ordinance No. 26, SG, issue 103/2008;
БДС 14776;
Ordinance No. РД-07-3, SG, issue 63/2014;
TS

	2
	Artificial lighting in work environment, premises of residential and public buildings, platforms of enterprises 
	New and/or existing sites and/or equipment
	Illumination
	Methodical guidelines on 
Measurement and evaluation of artificial lighting inside buildings
40-85, edition 
“Standardization” 1985
02-O Artificial Illumination control procedure

	Ordinance No 49, 
SG, issue 7/1976; 
Ordinance No 2, 
SG, issue 15/2007; 
Ordinance No 3, 
SG, issue 15/2007; 
Ordinance No 9, 
SG, issue 46/1994;
Ordinance No 24, 
SG, issue 95/2003; 
Ordinance No. 26, 
SG, issue 103/2008; БДС EN 12464-1: 2021; 
TS 

	3
	Noise in work environment
	New and/or existing sites and/or equipment
	Daily level of noise exposure; Average weekly level of noise exposure; Peak level of noise pressure;







	БДС EN ISO 9612
(БДС ISO 1999);

03.1- III Noise control procedure
	Ordinance No. 6, SG, issue 70/2005; TS

	4
	Electric installations and facilities up to 1000 V
	New and/or
Existing sites and/or equipment


	Impedance of "phase-protective conductor" loop
	Procedure 08-Z on Impedance of contour “Phase – protected conductor” control
	Ordinance No. 3, SG, issue 90 and 91/2004;
Ordinance No 16-116, SG, issue 26/2008; TS

	5
	Electric installations and 
facilities of up to 1000 V
	New and/or 
existing 
sites and/or equipment
	Strength of protective earthing installations;
	Procedure 10-ZZ on resistance of protective earthing installations control
	Ordinance No. 3, SG, issue 90 and 91/2004;
Ordinance No 16-116,
SG, issue 26/2008; TS

	6
	Electric installations and 
facilities of up to 1000 V
	New and/or 
existing 
sites and/or equipment
	Strength of lightning- protective earthing installations;
	Procedure 11-MZZ on resistance of protective lightning earthing installations control
	Ordinance No. 4, SG, issue 6/2011; TS










	
	
	
	
	
	

	
	
	
	
	
	

	7
	Noise inside the premises of residential and public buildings 
	New and/or 
existing 
sites and/or equipment
	Equivalent noise level;
Noise level
	БДС 15471;
Procedure 03-Ш Noise control procedure
	Ordinance No. 7, SG, issue 88/1999;
Ordinance No. 6, 
Appendix No. 2, table 1; SG, issue 58/2006; 

Ordinance No 9, SG, issue 46/1994; 

Ordinance No 26, SG, issue 103/2008; 
Technical Specification.

	


	
	
	
	
	



*The introduction of new versions of standards/documents or standards/documents that replace them is allowed. Up-to-date list of the standards/documents with their dated versions is provided by the Conformity Assessment Bodies.

Ordinance No. 3 on the design of electrical installations and power lines (SG, issue 90 and 91/2004); 
Ordinance No. 16-116 on the technical operation of energy equipment (SG, issue 26/2008); 
Ordinance No. 4 on the lighting protection of buildings, exterior equipment and outdoor spaces (SG, issue 6/2011); 
Ordinance No. 2 of the Ministry of Health on health requirements for computer and internet rooms for public use (SG, issue 15/2007); 
Ordinance No. 3 of the Ministry of Health on health requirements for kindergartens (SG , issue 15/2007); 
Ordinance No. 9 on health and hygiene requirements for the use of personal computers in education and extracurricular activities of students (SG, issue 46/1994); 
Ordinance No 24 on sanitary and hygienic requirements for nightclubs (SG, issue 95/2003); 
Ordinance No 26 on the structure and operation of crèches and children's meal provision centres and the health requirements for them (SG, issue 103/2008); 
Ordinance No. РД-07-3 on minimum requirements for the microclimate at workplaces (SG, issue 63/10.08.2014); 
Ordinance No. 6 on the minimum requirements towards occupational health and safety of workers when it comes to risks related to noise exposure (SG, issue 70/2005);
Ordinance No.7 on the minimum requirements for health and safety working conditions at the workplace and when using work equipment (SG, issue 88/1999);
Ordinance No. 6 on the noise indicators in environment that reflect  the discomfort degree during the various  time frames of the 24-hour period the limit values of noise indicators in environment.
Methods for assessment of the values of noise indicators and the harmful impacts of noise on population health (SG, issue 58/2006);
Ordinance No. 49 on artificial lighting of buildings (SG, issue 7/1976); 
Methodological guidelines for the measurement and evaluation of artificial lighting in buildings 40-85, Standartizatsia Publishing House, 1985 ;
TS – Technical specifications. 
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