
 ORDER 
  № А 54
Sofia, 30.01.2024 г.
Type C working conditions inspection body

at Elatsite – Med AD, Village of Mirkovo
                                        Management and office address: 

                                   2086 Village of Mirkovo, Sofia District

To perform inspection, according to the following scope:

	Scope type: flexible*

	No.
	Field of Inspection
	Control type
	Controlled parameter / characteristic:
	Test / measurement methods used in control; control procedure
	Regulations, standards, specifications, control schemes

	1
	2
	3
	4
	5
	6

	1. 
	Working and household environment microclimate
	New and/or operating sites /facilities/
	Air temperature;
Relative air humidity
Air flow velocity;
	CP No. 1.1
CP No. 1.2
CP No. 1.3
Ordinance No. RD-07-3 
SG, No. 63/2014 

БДС 16686
	Ordinance No. RD-07-3 
SG, No. 63/2014 

Ordinance No. 9 
SG, No. 46/1994 Ordinance No. 24 
SG, No. 95/2003 

Ordinance No. 2 
SG, No. 15/2007 
БДС 14776 
TС

	2. 
	Ventilation installations
	New and/or operating sites /facilities/
	Air flow velocity, air rate
	CP No. 9
БДС 12.3.018
	Ordinance No. 15 
SG, No. 68/2005
TC

	3. 
	Artificial lighting in working areas of residential and public buildings;
	New and/or operating sites /facilities/
	Illumination
	CP No. 2
Methodology for measurement of artificial lighting in buildings from Code of methods for hygiene requirements Volume IV
	Ordinance No. 9 
SG, No.  46/1994 

Ordinance No. 24 
SG, No.  95/2003 

Ordinance No. 49 
SG, No.  7/1976 
BSS EN 12464-1 
TC

	4. 
	Noise in working environment
	New and/or operating sites /facilities/
	Noise level,
Equivalent noise level,
Daily noise exposure level,
Average weekly noise exposure level;
Peak sound pressure level,
	CP No. 3.1
БДС EN ISO 9612 
/ БДС ISO 1999/
	Ordinance No. 6 
SG, No.  70/2005 

Ordinance No. 2 
SG, No.  15/2007 

Ordinance No. 24 
SG, No.  95/2003
TС

	5. 
	Noise in residential and public buildings premises
	New and/or operating sites /facilities/
	Noise level,
Equivalent noise level
	CP No. 3.2 
БДС 15471
	Ordinance No. 6 
SG, No.  58/2006, Annex 2, Table 1
Ordinance No. 2 
SG, No.  15/2007 

Ordinance No. 24 
SG, No.  95/2003
TС

	6. 
	Noise in working environment /In various territories and development areas in urban areas and outside them/
	New and/or operating sites /facilities/
	Noise level,
Equivalent noise level
	CP No. 3.2 
БДС 15471
	Ordinance No. 6 
SG, No.  58/2006, Annex 2, Table 2
TС

	7. 
	Vibrations transmitted to the hand-arm system
	New and/or operating sites /facilities/
	Daily vibration exposure value
	CP No. 4
БДС EN ISO 5349-1
БДС EN ISO 5349-2/А1
	Ordinance No. 3 
SG, No. 40/2005
TС

	8. 
	Air of the working environment
	New and/or operating sites /facilities/
	Dust concentration in the air of a working environment: – inhalable fraction – respirable fraction
Free crystalline silica
	CP No. 5.1
CP No.5.2
БДС EN 689+АС
БДС EN 482
БДС EN 481
БДС 2200
CP No. 6.3
БДС EN 689+АС
БДС EN 482
БДС EN 481
БДС 2200
БДС 2280
	Ordinance No. 13, 
SG, No.  8/2004

	9. 
	Air of the working environment
	New and/or operating sites /facilities/
	Concentration of chemical agents by linear colorimetric method with indicator tubes
	CP No. 6.1
БДС EN 689+АС
БДС EN 482
БДС EN 17621
	Ordinance No. 13 
SG, No.  8/2004

	10. 
	Water and sewage 
systems
	New and/or operating sites /facilities/
	Availability of documents and equipment Concentration of chemical agents
	CP No. 7
БДС EN 689+АС
БДС EN 482
БДС EN 17621
	Ordinance No. 9 
SG, No. 93 /2004 

Ordinance No.13 
SG, No.  8/2004
TС

	11. 
	Ionizing radiation
	New and/or operating sites /facilities/
	H*(10) equivalent dose rate
	CP No. 8
Ordinance on radiation protection
SG, No.  16/20.02.2018
	Ordinance on radiation protection 
SG, No. 16/20.02.2018

	12. 
	Electric assemblies and facilities with voltage up to 1000 V
	New and/or operating sites /facilities/
	Impedance of the “phase – protective conductor circuit”
	CP No. 10.1
	Ordinance No. 3
SG, No.  90 and 91/2004
Ordinance No. 16-116
SG, No. 26/07.03.2008
TС

	
	
	
	Insulation resistance
	CP No. 11.1
БДС  1986, section 3.3 (a), (b), (e) and (f)
	Ordinance No. 3
SG, No.  90 and 91/2004
Ordinance No. 16-116
SG, No. 26/07.03.2008
Ordinance No. 1 
SG, No.  46/2010
TС

	
	
	
	Safety fuse breakers SFB 
· trigger current 
· switch-off time 
· contact voltage
	CP No. 12.1
	Ordinance No. 3 
SG No. 90 and 91/2004 
Ordinance No. 16-116 
SG, No. 26/07.03.2008
Ordinance No. 1 
SG, No.  46/2010
TС

	13. 
	Electric assemblies and facilities up to 1000V and exceeding 1000 V
	New and/or operating sites /facilities/
	Resistance of lightning protection earthing systems
	CP No. 13.1
	Ordinance No. 4 
SG, No.  6/2011
TС

	
	
	
	Safety grounding systems resistance
	CP No.13.2
	Ordinance No. 3 
SG, No.  90 and 91/2004 
Ordinance No. 16-116 
SG, No. 26/07.03.2008
TС


*The introduction of a new version of standards/documents that replace them is allowed. An up-to-date list of standards/documents with their dated versions is provided by the CAB
Ordinance No. 9 RD-07-3 (SG, No. 63/2014) on the minimum requirements for the microclimate of workplaces;

Ordinance No. 3 on the structure of electrical installations and power lines, (SG. No. 90 and No. 91/2004, Amended, SG No. 42/2015);

Ordinance No. 16- 116 for technical operation of the energy equipment, (SG. No.  26/2008, as amended, SG No. 42/2015);

Ordinance No. 4 on lightning protection of buildings, exterior facilities and open spaces (SG, No.  6/2011);

Ordinance No. 1 of 27 May 2010 on the design, construction and maintenance of low-voltage electrical installations in buildings (SG No. 46/2010);

Ordinance No. 9 (SG, No.  46/1994) on the health and hygiene requirements for the use of personal computers in the education and extracurricular activities of students;

Ordinance No. 24 on the sanitary and hygienic requirements for discos (SG no. 95/2003);

Ordinance No. 15 of 28 July 2005 on technical rules and regulations for the design, construction and operation of the sites and facilities for the production, transmission and distribution of thermal energy (SG, No. 68/2005, amended SG No. 6/2016);

Ordinance No. 2 (SG, No. 15/2007) to the computer and internet rooms for public use; 

Ordinance No. 49 on artificial lighting in buildings (SG No. 7/1979, as amended, SG No. 64/1976);

Ordinance No. 6 (SG, No. 70/2005) on the minimum requirements for ensuring the health and safety of workers in case of risks related to noise exposure;

Ordinance No. 6 of 2006 (SG. No. on ambient noise indicators taking into account the degree of discomfort during different parts of the day, the limit values of ambient noise indicators in the premises of residential and public buildings, in areas and territories intended for residential construction, recreational areas and territories and mixed-use areas, the methods for assessing the values of noise indicators and the harmful effects of noise on the health of the population (title amended – SG No. 100/2021);

Ordinance No. 13 of 30 December 2003 on the protection of workers from risks related to exposure to chemical agents at work (SG No. 8/2004);

Ordinance No. 9 on ensuring safe and healthy working conditions in the operation and maintenance of water supply and sewerage systems (SG, No.  93/2004);

Ordinance No. 3 on the minimum requirements for ensuring the health and safety of workers in case of risks related to vibrations exposure (SG, No.  40/2005);

Ordinance on radiation protection SG No.. 16/20.02.2018

TС – Technical specification
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